**Single phase multi-rate meter**

|  |  |  |
| --- | --- | --- |
| Yueqing Kailai meter co., Ltd. | Technical Parameters: | Type:DDSF198  Connection：1Phase 2 Wire  Rated Current：5/60A  Rated Voltage：220 V  Voltage Range：75%Un ～ 120%Un  Frequency：50 Hz  Accuracy Active：1.0  IP 54  Voltage Circuit：≤2 watts，≤10VA  Current Circuit：<0.5 VA  Operating Temperature：-30℃～+55℃  Operating Temperature：-40℃～+70℃  Relative Humidity：≥ 95% no condensing  Starting Current：0.4% Ib  Minimum registered road current:20MA  Maximum creap current:10ma |
| |  |  | | --- | --- | | Functions and Features: | 1. Real Time 2. Date 3. Cumulative Active energy import reading(A -A kWh) 4. Last Bill Active Forwarded energy 5. RTC support: 10 years battery working life 6. Last Bill Maximum demand (kW) 7. Billing period counts，data store 12 month 8. Instantaneous phase voltage, current,PF, active power 9. Maximum demand kW for Current month 10. Supply Frequency 11. Traiff:4 12. Communication with IR and RS485（Hand hold unit, power off, programming, MD resetting, Time Setting） 13. Digital 8 14. LCD Display blue light 15. Meter No. | | | |