* serial number digital 1 phase shall be start from 16-07-XXXXXX
* 表号为16-07-000001 – 16-07-010000
* total not more than ten digit
* 合计不超过10位数
* Each meter shall be composted as flow : 每个表应包含如下内容
* number of phases and wires 相和线的数量
* country of manufacture 制造国家
* type designation 型号
* year of manufacture 制造年份
* unit of measurement 计量单位
* reference voltage, frequency 参比电压、频率
* rated basic and maximum Current 基本电流和最大电流
* meter constant (imp/kWh) 电表常数(imp/kWh)
* class index of meter 精度等级
* label " ຊັບສົມບັດຂອງ ຟຟລ ,ຟຟລ ສາມາດເຂົ້າກວດກາສ້ອມແປງ ປ່ຽນຖ່າຍ ແລະຍົກຍ້າຍໄດ້
* Bar code 条码
* EDL Logo

**Note**

* Printing nameplate by indelible ink 铭牌要用不可磨灭的墨水印刷
* All letters without notification are in black color and use font style Arial narrow 所有字体用黑色和Arial narrow字体
* For the Lao Language shall be use Phetsarath OT font 老挝语用Phetsarath OT 字体
* meter in the box shall be have the brochure in the box for each meter 每个表要单独装一个盒子，并配上使用手册
* EDL Logo shall be Color EDL logo按照上图的颜色

For the display 显示

上电情况下：

1. shall be show Two value Auto scroll every 5s 自动轮显，以下两项内容，间隔5S

End of billing that mean Total energy 1th 00h

截止本月1日0时的上月电量

Accumulate energy that mean Total Energy now

累计总电量

1. Button press 按键显示
2. Date and time shall be set Laos time Zone (UCT+07:00)Bangkok,Hanoi,jakata

日期和时间，老挝时区

1. Current (A)电流
2. Voltage (V)电压
3. End of billing ( Total energy fist moth at 00h

截止本月1日0时的上月电量

Accumulate energy (Now use how much) 累计总电量

1. PF mean cos🛇 功率因素

掉电情况下：

掉电情况下熄屏，可以按键激活显示

End of billing that mean Total energy 1th 00h

截止本月1日0时的上月电量

Accumulate energy that mean Total Energy now

累计总电量

无操作30S 重新熄屏

ຖະໜົນມິດຕະພາບລາວ-ໄທ, ຕູ້ ປ.ນ 309, ບ້ານ ທົ່ງກາງ, ເມືອງ ສີສັດຕະນາກ, ນະຄອນຫຼວງວຽງຈັນ ສປປ ລາວ

ໂທ: (856-21) 451537, 316094 - 1508. ແຟັກ: (856-21) 416381, 316128

ອີເມລ: [edldo@edl.com](mailto:edldo@edl.com); ເວັບໄຊ: www.edl.com.la